■. 품 명 : DOME CAMERA

1. 기   능

- 1/2.8” Sony 2.16M Pixels STARVIS CMOS

- H.264, H.265, MJPEG Triple Codec, Onvif Profile S(17.12v)

- High Performance Triple Streaming

- Day/Night with ICR, Min. 0.01Lux, LED on: 0Lux

- 2.8~12mm Mega Pixel DC Auto Iris Lens

- Motion Detection, Privacy Masking (4), Digital Zoom, Defog, 3DNR, LDC

Video Rotation (Corridor), WDR, SHDR, BLC

- Audio (1/1), Alarm (1/1), SD Slot (Max. 256GB)

- Built-In High Effective 30LEDs(IR Distance 30m)

- Option: PoE, 2Motors(2.8-12mm)

2. 기기 특성

- Image Sensor	: 1/2.8” 2.16M Sony STARVIS CMOS

- Minimum illumination	: Color:0.1Lux, 0.01Lux with Sens-Up(10x)/F1.2, 50IRE,LED On:0Lux

- Day & Night	: Day & Night with ICR (TDN)

- S/N Ratio	: More than 54dB (AGC Off)

- Lens	: 2.8 ~ 12mm 2M Varifocal Lens

- Iris	: DC Auto Iris

- Video Compression	: H.265 Main profile, H.264(High, Main, Base line profile), MJPEG

- Ethernet	: RJ-45(10/100BASE-T)

- Video Resolution	: Stream1:1920x1080, 1280x720, 960x540, 640x480, 640x360

Stream2:1280x720~320x240,

Stream3:640x480, 320x240

- Memory	: SD Slot SDHC/SDXC(256G)

- Client Viewer	: Web viewer

- Max. User Connection	: 10 Users

- Network Protocol	: TCP/IP, HTTP, HTTPS, UPnP, RTSP, DHCP, STATIC IP, Onvif

- IR Range	: 30m (30 IR LEDs)

- Operating Humidity	: 30 % ~ 90 % RH

- Operating Temp.	: -10°C~60°C(14°F~140°F)

- Power Consumption	: Max 7.5W

- Power Supply	: DC12V±10,

- Construction	: Plastic Body, PC bubble

- Dimension	: 130(W)mm x 107(H)mm x □100(Bubble)

- Weight About	: 0.5Kg

- Certificate	: CE, FCC, KC