■. 품 명 : BULLET CAMERA

1. 기   능

- 1/2.8” Sony 2.16M Pixels STARVIS CMOS

- H.264, H.265, MJPEG Triple Codec, Onvif Profile S(17.12v)

- High Performance Triple Streaming

- Day/Night with ICR, Min. 0.06Lux, LED on: 0Lux

- 2.8~12mm Mega Pixel DC Auto Iris Lens

- Motion Detection, Privacy Masking (4), Digital Zoom, Defog, 3DNR, LDC

- Video Rotation (Corridor), WDR, SHDR, BLC

- Audio (1/1), Alarm (1/1), SD Slot (Max. 256GB)

- Built-In High Effective POWER LEDs(IR Distance 40m)

- Option: PoE, 2Motors(2.8-13.5mm)

2. 기기 특성

- Image Sensor	: 1/2.8” 2.16M Sony STARVIS CMOS

- Scan mode	: Progressive Scan

- Number of effective pixels	: 1945(H) x 1097(V) approx. 2.13M pixels

- Minimum illumination	: Color:0.06Lux(x4) / F1.2, 50IRE, B/W: 0Lux (LED On)

- Day & Night	: Day & Night with ICR (TDN)

- S/N Ratio	: More than 54dB (AGC Off)

- Lens	: 2.8 ~ 12mm 2M Varifocal Lens H:108.5°(W)-32.2°(T),V:56.2°(W)-18.2(T),D:132.8°(W)-36.8°(T) Option: 2.8 ~ 13.5mm 5M Varifocal Lens H:99.1°(W)~30.3°(T),V:52.4° (W)~17.0°(T),D:118.2°(W)~34.8°(T)

- Iris	: DC Auto Iris

- Video Compression	: H.265 Main profile, H.264(High, Main, Base line profile), MJPEG

- Ethernet	: RJ-45(10/100BASE-T)

- Video Resolution	: Stream1:1920x1080, 1280x720, 960x540, 640x480, 640x360

Stream2:1280x720~320x240, Stream3:640x360, 320x240

- Video Streaming	: Simultaneously H.265/4 and MJPEG(Triple Codec)

- Video Frame Rate	: Up to 25/30fps@2M

- Bitrate Control	: CBR or VBR(200K~7Mbps)

- Audio	: Audio In/Out(1/1),Two Way(AAC,G.711 u-law,G.711 a-law)

- Memory	: SD Slot SDHC/SDXC(256G)

- Event	: Input: Sensor/Motion

Output :Sensor Output/SD Recoding

- Client Viewer	: Web viewer

- Max. User Connection	: 10 Users

- Network Protocol	: TCP/IP, HTTP, HTTPS, UPnP, RTSP, DHCP, STATIC IP, Onvif

- Image Quality	: Brightness, Contrast, Saturation, Hue, Sharpness, Denoise, 3DNR, Gamma, Defog

- Exposure	: Compensation, DC Iris, DSS, Anti-Flicker, Shutter Speed, AGC

- Back Light	: BLC, WDR, SHDR

- White Balance	: Manual, Auto, Day/night, Cloudy, Tungsten, Sunset

- Day & Night Mode	: Auto, Day, Night, EXT(cds), EXT(Low), EXT(High), Schedule

- Privacy / Motion	: 4Zones / Zones

- SD Card Recording mode	: Continuous, Motion, Sensor, Motion+Sensor

- LDC/Flip(Vertical/Horizontal)	: On / Off

- Video Rotation(Corridor)	: Off / 90 degree / 270 degree

- IR Range	: 40m (POWER IR LEDs)

- Operating Humidity	: 30 % ~ 90 % RH

- Operating Temp.	: -30°C~60°C(-22°F~140°F)

- Power Consumption	: Max 9.9W

- Power Supply	: DC12V±10, 1.5A

- Construction	: Aluminum body, Glass Window

- Dimension	: 120(W)mmX101(H)mmX285(D)mm

- Weight	: About 1.5Kg

- Certificate	: CE, FCC, KC, IP67