■. 품 명 : SPEED DOME CAMERA

1. 기   능

- 1/2” PS-CMOS 2M IP IR PTZ Camera

- Max.1080p@30/25fps¸H.264 Compression with Ambarella Codec

- Optical 36x Zoom, Digital 32x Zoom, Auto Focus

- Day & Night with ICR, Low up to 0.002Lux with DSS, LED On: 0Lux

- WDR, DIS, 3D DNR, Motion Detection, Privacy Masking (8), Defog, Time Schedule

- Preset(250), Group(12), Tour, Trace, Alarm(1/1), Dehumidification

- Max. IR Distance 400m (10pcs High Power LEDs + 4pcs Laser LEDs)

- Outdoor Type(IP66), Fan/Heater

2. 기기 특성

- Image Sensor	: 1/2” 2Mega Sony CMOS

- Scan mode	: Progressive Scan

- Total number of pixels	: 1,952(H) x 1,241(V), 2.4M Pixels

- Number of active pixels	: 1,937(H) x 1,097(V), 2.1M Pixels

- Resolution	: 1080P

- Minimum illumination	: Color : 0.15Lux , BW : 0.01Lux, LED On:0Lux

Min. Color 0.0375Lux, B/W 0.002Lux with DSS

- Video Output	: LAN / CVBS : 1.0Vp-p, 75Ω Composite

- S/N Ratio	: 50dB

- Lens	: 6 ~216mm(F1.5~F4.8)

Optical(36x), Digital Zoom(32x), Total Zoom (1152x)

- Focus mode	: Auto / Manual / Oneshot

- Angle of view	: D:65.56°~2.45°, H:58.44°~2.10°, V:34.11°~1.21°

- Hardware	: Flash (32Mbyte), RAM (256Mbyte)

Ethernet: RJ-45(10/100BASE-T)

- Video Output	: Channel 1ch (CVBS)

Compression H.264, MJPEG Dual Codec

FULL HD(1920X1080),HD(1280X720P),

VGA(640X480),QVGA(320X240)

Max. Frame rate 30/25fps

Bitrate control : CBR or VBR(64K~12Mbps)

- Audio	: Audio In(1), Audio Out(1),8 bit PCM (G711 u-law) 8Khz, Mono

- Memory Slot	: SD/SDHC Memory Slot

- Event	: Alarm / Motion Detection : E-mail, FTP, Event, Noti- Service

- Recording	: Manual / Schedule / motion Detection / Sensor Event

- Client Viewer	: Web viewer, CMS

- Network Protocol	: HTTP, TCP/IP, UDP, ARP, ICMP, RTP/RTSP/ DHCP, Telnet,

FTP, ,NTP, DDNS, SMTP, UPNP, PPPoE, Onvif, PSIA

- Pan/Tilt angle	: 360° Endless / -10°~ 92°

- Pan Speed	: 0.1° ~ 120°/sec (64 Levels), Preset: 240°/sec

- Preset point	: 250 Presets

- Alarm in/out	: 1 Inputs / 1 Relay Output

- Day & Night	: Day / Auto Slow / Auto fast / Night

- Back Light	: Off / WDR / HLC / BLC

- White Balance	: Auto / Indoor / Outdoor

- DNR	: Off / Low / Middle / Max

- Privacy / Motion	: 8 Zones / 1 Zones

- Stabilizer	: On/Off

- Defog	: Off/Auto/Manual

- IR Distance	: Max. 400m: 10pcs High Power LEDs+4pcs Laser LEDs

- Operating Humidity	: 30 % ~ 90 % RH

- Operating Temp.	: - 50°C to 50°

- Power Consumption	: Max 42W

- Power Supply	: AC24V, 50/60Hz

- Construction	: Aluminum body(Ivory/Black) & Plastic Window(Black)

- Dimension	: 238mm(W)X352(H)mm

- Weight About	: 5Kg (Camera Only)

- Certificate	: CE, FCC, KC, IP66, IK10