■. 품 명 : BULLET CAMERA

1. 기   능

- 1/2.0" CMOS Image Sensor

- 야간 초저조도 기능

- 지능형 이미지 프리셋 기능

- 최대 줌(Optical x18 / IP x10)

- 최대 60fps@1920x1080

-  쿼드 스트리밍 지원(Pri : H.265/H.264, Sec x3 : H.265/H.264/MJPEG)

- 야간 최대 가시거리 최대 80m 지원

- 지능형 영상분석 기능

- IVA : 가상선/영역, 출입 감지, 배회, 방향 감지, 발생/소멸 감지 등

- 분석 이벤트 : 디포커스 감지, 움직임 감지, 템퍼링, 오디오 감지

2. 기기 특성

- Sensor	: 1/2.0" CMOS Image Sensor

- Zoom	: Optical 18x

- focal length	: f = 6.8 ~ 122.4mm

- Angle of view	: Horizontal : 55.1°(wide) ~ 3.0°(tele), Vertical : 32.8°(wide) ~ 1.7°(tele)

- Maximum aperture ratio	: F1.6 ~ F2.8

- Focus comtrol	: Oneshot AF

- Lens type	: DC auto iris

- Min illumination	: Color : 0.0075 Lux(1/30sec, 35IRE) / BW : 0 Lux(IR ON)

- Electronic shutter speed	: 1/1 ~ 1/100,000 sec

- Day & Night	: Day / Night / Auto

- Back light compensation	: BLC / HLC / WDR

- Wide dynamic range	: 120dB

- White balance	: Auto tracing white / Auto white / Manual

- Gain Control	: Auto

- Noise reduction	: Auto / Manual

- Image stabilization	: Support

- Defog	: Support

- Image rotation	: Horizontal(Mirror), Vertical(Flip)

- Motion detection	: 8 regions on 23x15 cells

- Privacy masking	: 8 regions (polygons of 8 points)

- IR LED	: 8 pieces, max 80m

- Video analytics	: Motion detection, Intrusion detection, Line crossing detection, Video face detection, Camera tampering detection

- Burn-in-OSD	: Camera title, Direction, User-defined, Multi-lingual (English, Korean, French, German, Spanish, Italian, Russian, Japanese

Swedish, Portuguese, Dutch, Hungarian, Finnish, Special Symbols)

- Compression	: H.264 / H.265 / MJPEG

- Frame rate	: Max 60fps @ 1920x1080

- Bitrate control	: H.264/H.265 : CBR / VBR / Hybrid, MJPEG : VBR

- Resolutions	: 1920x1080 ~ 352x240

- Streaming	: Quad Streaming

Primary : H.264 / H.265, Secondary x 3 : H.264 / H.265 / MJPEG

- Compression	: G.711 u-law

- Sampling rate	: G.711 : 8KHz

- Bitrate	: G.711 : 64Kbps

- Streaming	: Full-duplex

- Input & Output	: 1 x Line-In (mono), 1 x Line-Out (mono)

- Event sources	: Video analytics, Audio detection, Client disconnection, Sensor input, User-defined event

- Event actions	: E-mail notification, OSD alert, FTP upload, PTZ preset, Alarm control, Recording, HTTP action

- Interface	: Ethernet 10/100/1000 base-T (RJ-45)

- Protocol	: IPv4/v6, TCP, UDP, IGMP(Multicast), ICMP, DHCP, HTTP, HTTPS, RTP, RTSP

FTP, SNMP, SMTP, UPnP, WS-Discovery, Zero Configuration, NTP, DDNS, RTMP

- Security	: Basic/Digest authentication, HTTPS, IP address filtering, User access log, TTA certification

- Application programming interface : ONVIF, PSIA, MPEG-TS

- Power supply	: Min DC 12V/1.5A, PoE(Power over Ethernet) : 802.3af

- Power consumption	: DC12V/PoE : Max 18W

- Operating condition	: -20°C ~ 70°C / Less than 90% RH

- Storage condition	: -50°C ~ 60°C / Less that 95% RH

- Certifications	: IP67, IK10, KC

- External devices	: 1 x Sensor-In (dry contact, NO/NC)

1 x Alarm-Out (dry contact, NO)

1 x RS-485 port : Z/F control etc.

- Edge storage	: Micro SD/SDHC/SDXC (Max 512GB)

- Color/Material	: Body : Gray / Aluminium

Head : Gray / Aluminium

- RAL code	: White : TBD`

: Black : TBD

- Dimension	: Ø108 x 391.5mm

- Weight	: 1,551 g